**Notice to Tenderers No:** 3

Banana Shire Council (BSC) has received a query with respect to the Tender. The following has been reviewed:

**Additional Information**

Banana Shire Council has identified and updated the following information:

Question-1: What is the prime treatment, as spraying SAMI onto the profiled/ gravel surface isn’t suitable?

SAMI Seal design (binder rate) to be determined by the tendered/seal designer. Intention to act as a waterproofing layer between the underlying existing and the new on top.

The layer is between the existing surface, profiled and non-profiled sections and the Asphalt corrector layer. SAMI is to be designed with a minimum binder application rate of 1.8L/m2. **Alternative treatments may be proposed by the tenderer.**   
  
Question-2: Confirm the corrector layer will be sprayed with C170 bitumen to assist with adhesion of the HateLit C?

In line with clause 1.3.1 & 1.6.2, Appendix G. C170 is preferred however, C320 shall be considered if the grid will be placed in warm/summer conditions.   
  
Question-3: Should profiling be completed at 45mm to allow for the thickness of the 10mm SAMI seal?

Profiling should make allowance for matching into the existing surface at the interface with the concrete edge beam. 40mm is a nominal depth with tolerance (+-5mm), as site conditions dictate should be allowed for.

**Tender Submission**

Tender Response and attachments will be accepted via email submission to [tenders@banana.qld.gov.au](mailto:tenders@banana.qld.gov.au) or via Dropbox. Hard Copies are not required.

**Dated: 15th August 2025**