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T2627.12 DRFA Program Kooingal Court Reconstruction						
Notice to Tenderers

NOTICE TO TENDERERS NO:		2		

Banana Shire Council (BSC) has received a query with respect to the Tender. The following has been reviewed:



Question: Does the Cul-de-sac currently have seal on it , or has council profiled the site and removed it. If it is currently sealed is the removal to be included in the first pay item of pavement reconstruction.



Answer:
The Site is able to be reviewed freely and unimpeded by tenderers and is currently spray sealed, with failed sections.
The line item from thew BOQ: Reconstruct unbound granular pavement. Excludes seal is referred to in the QRA Treatment Guide, and the Technical Specification for the works.

[bookmark: x__Toc242427605]Extract from Section 7. BITUMINOUS and ASPHALTIC PAVEMENT REPAIR TREATMENTS of the Technical Specification:
 
[bookmark: x__Toc242427606]7.1 General
The Contractor shall supply all materials, plant, labour, testing and supervision necessary to complete the bituminous and asphaltic works in accordance with the Contract, approved seal design and relevant MRTS specifications.
The works shall include preparation and acceptance of the pavement surface, supply and application of bituminous binder, spreading and rolling of cover aggregate, sweeping, testing, traffic management and rectification of nonconforming works.
 
[bookmark: x__Toc242427607]7.2 Subgrade Improvement Works
 
7.2.1 General
The Contractor shall undertake excavation, subgrade preparation, supply and installation of geotextile, geogrid and rockfill in accordance with the approved drawings, MRTS04, MRTS27 and the project-specific requirements of this specification.
Where geogrid reinforcement is required, the applicable provisions of MRTS58 shall also be considered and incorporated into the contract specification.
 
7.2.2 Material requirements
Rockfill shall comprise sound, durable, clean crushed or quarried rock, nominally 50–100 mm in size, free from excessive fines, organic material, clay contamination and deleterious substances.
Geotextile shall be BIDIM 64 or an approved equivalent. Geogrid shall be Tensar InterAx NX850 or an approved equivalent supported by engineering evidence demonstrating equivalent performance.
The Contractor shall submit material source information, test certificates, product data sheets and installation recommendations before commencing work.
 
7.2.3 Excavation and subgrade preparation
The Contractor shall excavate failed pavement and unsuitable material to the approved limits and formation levels.
The exposed subgrade shall be assessed for stability, bearing capacity, moisture condition, soft spots, pumping and groundwater.
Where conditions differ materially from the design assumptions, the Contractor shall notify the Superintendent and obtain direction before proceeding.
 
[bookmark: x__Toc242427608]7.3 Pavement
 
7.3.1 General
The Contractor shall supply, place, compact, test and finish the granular pavement layers in accordance with MRTS05 Unbound Pavements and the approved drawings.
The pavement shall comprise 125 mm Type 2.3 subbase and 125 mm Type 2.1 base, each measured as compacted thickness.
 
7.3.2 Material compliance
HP-02
Granular pavement materials shall comply with the applicable MRTS05 material subtype requirements.
The Contractor shall submit laboratory test results and material compliance documentation for grading, plasticity, moisture-density characteristics and other properties required by MRTS05.






Tender Submission

Tender responses and attachments will be accepted via email submission to  tenders@banana.qld.gov.au or VendorPanel. Hard Copies are not required.




Dated: 9th November 2026
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